
0. <WINNT.31>: It contains drivers for Windows NT V3.1 to support " > 16MB "
   system memory that is not supported by AHA 154x driver. The following is
   its content:

        0.1. OEMSETUP.INF: Setup Information File
        0.2. DCSCSI.SYS  : SCSI Driver
        0.3. DCSCSI      : Setup Tag File

             [Before Driver Installation]
             Since your SCSI adapter is AHA 154x driver compatible, the
             operating system would see it as an 154x adapter and
             automatically use AHA 154x driver to work with your adapter when
             installing the operating system. It's O.K. to use AHA 154x driver,
             but not for the environment that equips with system memory over
             16MB. For this case, you must install the driver shipped along
             your adapter to overcome this problem that isn't supported by 154x
             driver. The folloeing are the details for Driver Installation &
             Removal.


             [Driver installation]

                0. Enter the "Main" screen & select the "Windows NT Setup" icon
                   to proceed.

                1. Enter the "Options" & select "Add/Remove SCSI Adapters..."
                   for further operation.

                2. You may see it shows "Adaptec 154x/164x". This is because
                   your adapter is 154x driver compatible & recognised as one
                   of that kind.

                3. Choose "Add" and move to select "Other" in the "Select SCSI
                   Adapter Option" for adding driver from driver diskette.

                4. Insert the driver diskette in the proper drive (A: or B:)
                   and click the "OK" icon. The "Select OEM Option" screen
                   should display message like "SCSI Adapter for DC-8X0/3X0".
                   Then go on click the "Install" icon, the system would
                   preoceed installing the driver from floppy disk.

                5. Re-enter the "Options" & select "Add/Remove SCSI
                   Adapters..." to remove the "Adaptec 154x/164x" driver by
                   clicking the "Remove" icon and leave the newly installed
                   driver to work with your adapter.

                6. Shutdown the system & re-boot to complete the Driver
                   Installation.

             [Driver removal]
             To remove the driver, you can follow the procedures:

                0. Enter the "Main" screen & select the "Windows NT Setup" icon
                   to proceed.

                1. Enter the "Options" & select "Add/Remove SCSI Adapters..."
                   for further operation.

                2. You may see it shows "DC-8x0/3x0".

                3. Choose "Add" and move to select "Adaptec 154x/164x" in the
                   "Select SCSI Adapter Option" for adding driver to replace
                   the adapter's driver, which is going to be removed.

                4. Then select the "DC-8x0/3x0" and move on to choose "Remove"
                   icon to complete the Driver Removal.

                5. Shutdown your NT system and re-boot, the Adaptec 154x/164x
                   driver would be loaded and used from now on.

