Release Notes	04-Oct-1994

1. Product Name and Revision Level

SKFINT.SYS v2.10        

2. Product Description

SKFINT.SYS is the driver for the SK-NET FDDI ISA adapter
under the first release of Windows NT on Intel processors.

The driver corresponds to the NDIS 3.0 Specification as delivered with
the first release of the Windows NT DDK.

3. Release Status

This is the final version. There are no restrictions on shipment. 

4. Release Notes

Enjoy.

5. Test Results

Installed version of Windows NT: 3.1, Build 518 (September 1993)

Microsoft Test Suite with
	Server	Compaq 486/33m with
			SK-NET FDDI EISA adapter as trusted card

		Client	Compaq 486/33m with
			SK-NET FDDI ISA adapter as test card
			SK-NET FDDI EISA adapter as trusted card

TCP/IP and FTP on FI
(CAUTION: CONFIGURE ONLY ONE ADAPTER TO BE USED BY TCP/IP!)
	Ping between computers running Windows NT ok.
	Ping, File Get and Put from a DOS client using ETHDRV over UPPSPD ok
	(TOKDRV over UPPSLW failed - perhaps because ARP HwType is incorrect).

6. Description of New Features

None.

7. List of Problems Fixed

v2.00 Rev. A
  - OID_GEN_DRIVER_VERSION now returns NDIS version (3.00) instead of driver
    version.
  - On EISA and MCA machines the installation script inserts the keyword
    <BusNumber> into the registry.
  - More memory is used as receive buffer to reduce overflows.
v2.00 Rev. C
  - Fixed test for successful memory allocation.
v2.00 Rev. D
  - Runs on multiprocessor systems.
  - LINK_SPEED reporting corrected.
v2.01
  - Rejecting unsupported filters.
v2.10
  - Included EnhancedNonLlc mode.
  - Implemented	limited promiscuous mode (receive all NON-LLC frames).
    This may be disabled by setting <LimitPromiscuous> to 1 in the registry.
  - Runs stable on multiprocessor systems.

8. Known Limitations

None.
