;***********************************************************************
;
; OEMSETUP.INF
;
;       Intel EtherExpress PRO Ethernet Adapter and driver SETUP INF file.
;
;***********************************************************************

;-----------------------------------------------------------------------
; OPTION TYPE
; -----------
; This identifies the Option type we are dealing with.  The different
; possible types are:
;
; COMPUTER, DISPLAY, MOUSE, KEYBOARD, LAYOUT, SCSI, PRINTER, ...
;
;  Types specific to networking:
;
; NetAdapter,        a netcard / adapter combination or just a netcard
; NetDriver,         just a netcard driver
; NetTransport,      a complete NDIS-compliant TDI transport stack
; NetService,        an NT networking service
; NetWork,           a complete network ensemble.
; NetProvider        a complete network which supports NT MPR protocol
;-----------------------------------------------------------------------

[Identification]
    OptionType = NetAdapter

;-----------------------------------------------------------------------
; PlatformsSupported
; ------------------
; This identifies the platforms supported by the adapter card.
; Possible types are:
;
; ISA, EISA and MCA
;-----------------------------------------------------------------------

[PlatformsSupported]
    ISA
    EISA
;    MCA
    "Jazz-Internal Bus"

;-----------------------------------------------------------------------
; LANGUAGES SUPPORTED
; -------------------
;
; The languages supported by the OEM INF, For every language supported
; we need to have a separate text section for every displayable text
; section.
;
;-----------------------------------------------------------------------

[LanguagesSupported]
    ENG

;-----------------------------------------------------------------------
; OPTION LIST
; -----------
; This section lists the OEM Option key names.  These keys are locale
; independent and used to represent the option in a locale independent
; manner.
;
;-----------------------------------------------------------------------

[Options]
    EPRONT

;-----------------------------------------------------------------------
; OPTION TEXT SECTION
; -------------------
; These are text strings used to identify the option to the user.  There
; are separate sections for each language supported.  The format of the
; section name is "OptionsText" concatenated with the Language represented
; by the section.
;
;-----------------------------------------------------------------------

[OptionsTextENG]
    EPRONT = "Intel EtherExpress(TM) PRO Ethernet Adapter"


[Files-Inf]
1, oemsetup.inf, SIZE=50000, RENAME=$(!UG_Filename)


[Files-EPRONT]
1, EPRONT.SYS, SIZE=50000

[Files-hlp]
1, EEPRO.HLP, SIZE=14295

;***********************************************************************
; CONSTANTS FOR USING DIALOGS
;***********************************************************************

[FileConstants]
;
;  File names, etc.
;
UtilityInf      = "UTILITY.INF"
ParamInf        = "NCPARAM.INF"
subroutineinf   = "SUBROUTN.INF"
SoftwareType    = "driver"
Exit_Code       = 0

;
; EventLog Message File
;
NetEventDLL     = "%SystemRoot%\System32\netevent.dll"
IoLogMsgDLL     = "%SystemRoot%\System32\IoLogMsg.dll"

; Product Info
;
Manufacturer    =  "Intel"
ProductMajorVersion     = "1"
ProductMinorVersion     = "0"
ProductVersion  = $(ProductMajorVersion)"."$(ProductMinorVersion)
;
; Software
;
ProductSoftwareName     = "EPRO"
ProductSoftwareTitle    = "Intel EtherExpress PRO Ethernet Adapter Driver"
ProductSoftwareImagePath = "\SystemRoot\System32\drivers\epront.sys"
NetRuleSoftwareType     = "eproSys ndisDriver eproDriver"
NetRuleSoftwareUse      = $(SoftwareType)
NetRuleSoftwareBindForm = """EPROSys"" yes no container"
NetRuleSoftwareClass    = {"eproDriver basic"}
NetRuleSoftwareBindable = {"eproDriver eproAdapter non exclusive 100"}
;
; Hardware
;
ProductHardwareName     = "EPRO"
ProductHardwareTitle    = "Intel EtherExpress PRO Ethernet Adapter"
NetRuleHardwareType     = "epro eproAdapter"
NetRuleHardwareBindForm = " yes yes container"
NetRuleHardwareClass    = {"eproAdapter basic"}
;
;  MicroChannel System ID Info
;
EE16_1BYTE      = 139
EE16_2BYTE      = 98
NETCARD_ID      = 25227
;
; Registry Key
;
ProductKeyName  = $(!NTN_SoftwareBase)"\"$(Manufacturer)"\"$(ProductSoftwareName)"\CurrentVersion"
ParamKeyName    = $(!NTN_ServiceBase)"\"$(ProductHardwareName)"\Parameters"

[ProductType]
STF_PRODUCT  = Winnt
STF_PLATFORM = I386

[GeneralConstants]
;
;  Program flow control variables.
;
from      = ""
to        = ""
;
;  Return codes; Exit_Code is set to one of these
;
ExitCodeOk     = 0
ExitCodeCancel = 1
ExitCodeFatal  = 2

KeyNull         = ""
MAXIMUM_ALLOWED   = 33554432
RegistryErrorIndex = NO_ERROR
KeyProduct      = ""
KeyParameters   = ""

TRUE            = 1
FALSE           = 0
NoTitle         = 0

ExitState   = "Active"
OldVersionExisted = $(FALSE)

DriverPath      = $(!STF_NTPATH)\drivers

;MachineType = ""

;***********************************************************************
; Language-Dependent Dialog Constants
;***********************************************************************

[FileConstantsENG]
;
;  Variables to support thermometer gauge and error dialogs
;
ProCaption   = "Windows NT Setup"
ProCancel    = "Cancel"
ProCancelMsg = "Windows NT Networking is not correctly installed.  "+
	       "Are you sure you want to cancel copying files?"

ProCancelCap = "Network Setup Message"
ProText1     = "Copying:"
ProText2     = "To:"


;
; Product Info
;
FunctionTitle = "Intel EtherExpress PRO Ethernet Adapter Setup"
;
; Software
;
ProductSoftwareDescription = "Intel EtherExpress PRO Ethernet Driver"
;
; Hardware
;
ProductHardwareDescription = "Intel EtherExpress PRO Ethernet Adapter"

;
; Dialog Message Information
;
IRQList = {"3", "5", "9", "10", "11"}
IOReadyList = { "Late", "Never" }
IOReadyListExt = { "Early", "Late", "Never" }
TransceiverList = {"Thick Net (AUI/DIX)","Thin Net (BNC/COAX)","Twisted-Pair (TPE)","Auto Connect"}
IOAddrList = ^(IOAddrChoices, 1)
IOAddrValues = ^(IOAddrChoices, 2)

[IOAddrChoices]
IOBase_1  = "0x300",768
IOBase_2  = "0x310",784
IOBase_3  = "0x320",800
IOBase_4  = "0x330",816
IOBase_5  = "0x340",832
IOBase_6  = "0x350",848
IOBase_7  = "0x360",864
IOBase_8  = "0x370",880
IOBase_9  = "0x200",512
IOBase_10 = "0x210",528
IOBase_11 = "0x220",544
IOBase_12 = "0x230",560
IOBase_13 = "0x240",576
IOBase_14 = "0x250",592
IOBase_15 = "0x260",608
IOBase_16 = "0x270",624
IOBase_17 = "0x380",896
IOBase_18 = "0x390",912
IOBase_19 = "0x3a0",928
IOBase_20 = "0x3b0",944
IOBase_21 = "0x3c0",960
IOBase_22 = "0x3d0",976
IOBase_23 = "0x3e0",992
IOBase_24 = "0x3f0",1008
IOBase_25 = "0x280",640
IOBase_26 = "0x290",656
IOBase_27 = "0x2a0",672
IOBase_28 = "0x2b0",688
IOBase_29 = "0x2c0",704
IOBase_30 = "0x2d0",720
IOBase_31 = "0x2e0",736
IOBase_32 = "0x2f0",752


[DialogConstantsENG]
;
; Common button names, etc.
;
Help        = "&Help"
Exit        = "Cancel"
OK          = "OK"
HelpContext = ""
Continue    = "Continue"
Cancel      = "Cancel"

[date]
    ; Now is a list which contains { Sec from 1-1-1970, Year, Month, Day, Hour,
    ; Minute, Second }
    Now = {} ? $(!LIBHANDLE) GetSystemDate

[Source Media Descriptions]
;    1  = "Intel EtherExpress PRO Driver Disk"  
    1  = "Intel EtherExpress PRO Driver Disk"  

;-----------------------------------------------
; Input DIALOGS
;-----------------------------------------------
[FileDependentDlgENG]

DlgType = "RadioCombination"
DlgTemplate = "EE_16"
Caption = $(FunctionTitle)

DlgText = "Please select values for the following fields:"

Combo1Label = "&Interrupt Number:"
Combo2Label = "I/O &Port Address:"
Combo3Label = "I/O &Channel Ready:"
Combo4Label = "&Transceiver Type:"

Combo1List = $(IRQList)
Combo1Out  = $(IRQValue)
Combo2List = $(IOAddrList)
Combo2Out  = $(IOAddrValue)
Combo3List = $(IOReadyList)
Combo3Out  = $(IOReadyValue)
Combo4List = $(TransceiverList)
Combo4Out  = $(TransceiverValue)
ComboListItemsIn  = {Combo1List, Combo2List, Combo3List, Combo4List}
ComboListItemsOut = {Combo1Out, Combo2Out, Combo3Out, Combo4Out}

EditTextIn = ""
EditTextLim = ""
CBOptionsGreyed = {}
NotifyFields = {NO, NO}

HelpContext = 1

;---------------------------------------------------------------------------
; 1. Identify
;
; DESCRIPTION:   To verify that this INF deals with the same type of options
;                as we are choosing currently.
;
; INPUT:         None
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL
;                $($R1): Option Type (COMPUTER ...)
;                $($R2): Diskette description
;---------------------------------------------------------------------------

[Identify]
    ;
    ;
    read-syms Identification

    set !G:DebugOutputControl = 1
 
    set Status     = STATUS_SUCCESSFUL
    set Identifier = $(OptionType)
    set Media      = #("Source Media Descriptions", 1, 1)

    Return $(Status) $(Identifier) $(Media)

;------------------------------------------------------------------------
; 2. ReturnOptions:
;
; DESCRIPTION:   To return the option list supported by this INF and the
;                localised text list representing the options.
;
;
; INPUT:         $($0):  Language used. ( ENG | FRN | ... )
;
; OUTPUT:        $($R0): STATUS: STATUS_SUCCESSFUL |
;                                STATUS_NOLANGUAGE
;                                STATUS_FAILED
;                                STATUS_NOTSUPPORTED
;
;                $($R1): Option List
;                $($R2): Option Text List
;------------------------------------------------------------------------

[ReturnOptions]
    ;
    ;
    set Status        = STATUS_FAILED
    set OptionList     = {}
    set OptionTextList = {}

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) in $(LanguageList)
	;
	; Check if the platforms requested is supported
	;
	ifstr(i) $($1) == ""
	    goto returnoptions
	endif

	set PlatformList = ^(PlatformsSupported, 1)
	Ifcontains(i) $($1) in $(PlatformList)
	    goto returnoptions
	else
	    set Status = STATUS_NOTSUPPORTED
	    goto finish_ReturnOptions
	endif
    else
	set Status = STATUS_NOLANGUAGE
	goto finish_ReturnOptions
    endif

    ;
    ; form a list of all the options and another of the text representing
    ;

returnoptions = +
    set OptionList     = ^(Options, 1)
    set OptionTextList = ^(OptionsText$($0), 1)
    set Status         = STATUS_SUCCESSFUL

finish_ReturnOptions = +
    Return $(Status) $(OptionList) $(OptionTextList)

;------------------------------------------------------------------------
;
; InstallOption:
;
;      This section is shelled to by main installation processing
;      or by NCPASHEL.INF during reconfig, removal, update, etc.
;
;
; FUNCTION:  To copy files representing Options
;            To configure the installed option
;            To update the registry for the installed option
;
; INPUT:     $($0):  Language to use
;            $($1):  OptionID to install
;            $($2):  SourceDirectory
;            $($3):  AddCopy  (YES | NO)
;            $($4):  DoCopy   (YES | NO)
;            $($5):  DoConfig (YES | NO)
;
; OUTPUT:    $($R0): STATUS: STATUS_SUCCESSFUL |
;                            STATUS_NOLANGUAGE |
;                            STATUS_USERCANCEL |
;                            STATUS_FAILED
;
;------------------------------------------------------------------------
[InstallOption]

    set !G:DebugOutputControl = 1
    ;
    ; Set default values for
    ;
    Debug-Output "At InstallOption"
    set Status   = STATUS_FAILED
    ;
    ; extract parameters
    ;
    set Option   = $($1)
    set SrcDir   = $($2)
    set AddCopy  = $($3)
    set DoCopy   = $($4)
    set DoConfig = $($5)

    ;
    ; Check if the language requested is supported
    ;
    set LanguageList = ^(LanguagesSupported, 1)
    Ifcontains(i) $($0) NOT-IN $(LanguageList)
	Return STATUS_NOLANGUAGE
    endif

    set-subst LF = "\n"

    read-syms GeneralConstants
    read-syms FileConstants

    read-syms DialogConstants$(!STF_LANGUAGE)
    ifstr(i) $(!NTN_Origination) == "NCPA"
	set Continue = "OK"
    endif
    read-syms FileConstants$(!STF_LANGUAGE)

    detect date

    set-title  $(FunctionTitle)

    set to   = Begin
    set from = Begin

    Set PlatformList = ^(PlatformsSupported, 1)
    Set MachineType = *($(PlatformList), $($R1))
    Debug-Output "BusTypeNum is: "$($R1)
    Debug-Output "MachineType is: "$(MachineType)

;
;  Assume all is well.
;
    set CommonStatus = STATUS_SUCCESSFUL

    EndWait

;
;   Set up the operation-mode-based variables and gaily welcome
;   the user.  If the "install mode" variable is improperly set,
;   assume this is a new installation.
;

Begin = +
    Debug-Output "At Begin"
    Set ActivateDetection = FALSE

    Ifstr(i) $(!NTN_InstallMode) == deinstall
	set StartLabel = removeadapter
    else-Ifstr(i) $(!NTN_InstallMode) == Update
	set StartLabel = UpgradeSoftware
    else-Ifstr(i) $(!NTN_InstallMode) == bind
	set StartLabel = bindingadapter
    else-Ifstr(i) $(!NTN_InstallMode) == configure
	set ActivateDetection = TRUE
	set StartLabel = configureadapter
		  ;
	; If MCA we cannot Configure, so just exit out.
	;       
	ifstr(i) $(MachineType) == "MCA"
	    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
		Debug-Output "Cannot configure the EtherExpress MCA driver software."
		Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
	    else
		Debug-Output "Cannot configure the EtherExpress MCA adapter card."
		Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_HARDWARE
	    endif
	    set Error = $($R0)
	    set from = end
	    set to = end
	    goto nonfatalinfo
	endif
	;
	;   You cannot config the software component
	;
	Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	    Debug-Output "Cannot configure the 82595 driver software."
	    Shell $(UtilityInf),RegistryErrorString,CANNOT_CONFIGURE_SOFTWARE
	    ifint $($ShellCode) != $(!SHELL_CODE_OK)
		Debug-Output "ShellCode error: cannot get an error string."
		goto ShellCodeError
	    endif
	    set Error = $($R0)
	    set from = end
	    set to = end
	    goto nonfatalinfo
	endif
    else
	set ActivateDetection = TRUE
	set StartLabel = installadapter
	set OEM_ABANDON_OPTIONS = {}
	set OEM_ABANDON_SOFTWARE = FALSE
	set OEM_ABANDON_ON = TRUE
    endif

    ;===================================================
    ;  Netcard Detection logic
    ;
    ;  Initialize use of netcard detection;
    ;  Construct require global parameter variables
    ;
    Debug-Output "OEMNADIN.INF: =================================================="
    Debug-Output "OEMNADIN.INF: STF_CWDIR is: "$(!STF_CWDIR)
    Debug-Output "OEMNADIN.INF: STF_LANGUAGE is: "$(!STF_LANGUAGE)
    Debug-Output "OEMNADIN.INF: Option is: "$(Option)
    Debug-Output "OEMNADIN.INF: !STF_NCDETECT  is: "$(!STF_NCDETECT)
    Debug-Output "OEMNADIN.INF: !STF_NCOPTION  is: "$(!STF_NCOPTION)
    Debug-Output "OEMNADIN.INF: !STF_NCDETCARD is: "$(!STF_NCDETCARD)
    Debug-Output "OEMNADIN.INF: !STF_NCDETINFO is: "$(!STF_NCDETINFO)
    Debug-Output "OEMNADIN.INF: MachineType is: "$(MachineType)
    Debug-Output "OEMNADIN.INF: =================================================="

    Set DetectedCard = FALSE

    Ifstr(i) $(ActivateDetection) != TRUE
	Goto $(StartLabel)
    Endif

    ifstr(i) $(MachineType) == "MCA"
	goto CheckForMCA
    endif

    set IRQValue = *($(IRQList), 2)
    set IOAddrValue = *($(IOAddrList), 1)
    set IOReadyValue = *($(IOReadyList), 1)
    set TransceiverValue = *($(TransceiverList), 4)

    Ifstr(i) $(!STF_NCDETECT) == YES
	Ifstr(i) $(!STF_NCOPTION) == $(Option)
	   Set DetectedCard = TRUE
	   Debug-Output "OEMNADIN.INF: Setting DetectedCard to TRUE"
	Endif
    Endif
    ;
    ;  End Netcard Detection logic
    ;===================================================


    Shell "" DebugConfiguration "After parameter querying"

    Set from = $(fatal)
    Set to = $(fatal)
    Goto $(StartLabel)

;-----------------------------------------------
; Installation Section
;-----------------------------------------------

installadapter = +
    Debug-Output "At installadapter"
;
;   First, check whether the same version of the software exists
;

    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct

    Ifstr $(KeyProduct) != $(KeyNull)
	;
	; Same version already existed in the local machine
	; Popup the dialog and ask the user whether he wants to continue
	;
	CloseRegKey $(KeyProduct)

	ifstr(i) !(NTN_RegBase) == $(ProductKeyName)
	   ;
	   ; Cannot Install the same software again
	   ;
	   Shell $(UtilityInf), VerExistedDlg, $(ProductSoftwareTitle),+
	       $(ProductVersion)
	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif

	   goto end
	else
	   ;
	   ; Add a new adapter card?
	   ;
	   Shell $(UtilityInf), CardExistedDlg

	   ifint $($ShellCode) != $(!SHELL_CODE_OK)
	       Debug-Output "ShellCode error: cannot get an error string."
	       goto ShellCodeError
	   endif

	   ifstr(i) $($R1) != "OK"
	       goto end
	   endif
	   set OldVersionExisted = $(TRUE)
	endif
    endif

    ; If we're installing a second time, don't re-copy the help file
    ; !!!
    ifint $(OldVersionExisted) == $(FALSE)
	ifstr(i) $(!NTN_InstallMode) == "install"
	   Ifstr(i) $(DoCopy) == "YES"
		Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) NO
	      
		Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		    Goto ShellCodeError
		Else-Ifstr(i) $($R0) == STATUS_FAILED
		    Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
		    ifint $($ShellCode) != $(!SHELL_CODE_OK)
			goto ShellCodeError
		    endif
		    set Error = $($R0)
		    Goto fatal
		Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
		    Goto successful
		Endif
    
		Set SrcDir = $($R1)
	    endif

	    install "Install-Helpfile"
	endif
    endif

    SetHelpFile "eepro.hlp" 1 6


    ;===================================================
    ;  Netcard Detection logic
    ;
    ;   If this is a detected card, query its parameters
    ;   and merge them into the default list.
    ;
    Ifstr(i) $(DetectedCard) != TRUE
	Goto adaptersetup
    Endif
    ;
    ;   Get the detected parameters
    ;
CheckForMCA = +    
    Debug-Output "At CheckForMCA"
    StartWait
    ;
    ;   Check to see if were on a MicroChannel Machine
    ;
    Shell $(UtilityInf), MCAFindBus, $(EE16_1BYTE), $(EE16_2BYTE)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "OEMNADIN.INF: Failed Return from MCAFindBus."
	goto CheckForISA
    endif
    ifstr $($R0) != "NO_ERROR"
    Debug-Output "OEMNADIN.INF: Failed Return from MCAFindBus."
	goto CheckForISA
    endif
    ifstr(i) $($R1) == {}
	set Error = $(CANNOT_FIND_ANY_CARD)
	set CommonStatus = USER_CANCEL
	set from = "end"
	goto nonfatal
    endif
    set AdapterList = $($R1)
    goto skipoptions

CheckForISA = +

    Debug-Output "At CheckForISA"
    Shell $(ParamInf) Param_QueryCard $(!STF_NCDETCARD)
    EndWait
    Ifstr(i) $($R0) != STATUS_SUCCESSFUL
	Goto adaptersetup
    Endif
    ;
    ;   Merge the detected values in.
    ;
    Set DetectedParams = $($R1)
    Debug-Output "OEMNADIN.INF: Calling Param_SetDefaults to merge detected params"
    Shell $(ParamInf) Param_SetDefaults $(DetectedParams)
    ;
    ;  End Netcard Detection logic
    ;===================================================

    goto adaptersetup

;-----------------------------------------------
; Configuration Section
;-----------------------------------------------
;
;   Get the current values of all the parameters
;
configureadapter = +
    Debug-Output "At configureadapter"
   
    SetHelpFile "eepro.hlp" 1 6

    Ifstr $(KeyProduct) == $(KeyNull)
	OpenRegKey $(!REG_H_LOCAL) "" $(!NTN_RegBase) $(MAXIMUM_ALLOWED) KeyProduct
	Ifstr $(KeyProduct) == $(KeyNull)
	    set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
	    Debug-Output "Cannot find component product key"
	    goto fatalregistry
	Endif
    Endif

    ;
    ; Get the other parameters;  they're attached to the service parameters key
    ;
    Debug-Output "INF: Shelling to FindService"
    Shell $(UtilityInf) FindService, $(KeyProduct)
    Ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "INF: FindService shell failure"
	Goto ShellCodeError
    Endif
    Ifstr(i) $($R0) != NO_ERROR
	Debug-Output "INF: FindService Shell error: "$($R0)
	Goto fatalregistry
    endif

    Set KeyParameters = $($R2)

    ;
    ;  We don't need the services key, so close it.
    ;
    CloseRegKey $($R1)

    Ifstr $(KeyParameters) == $(KeyNull)
	set RegistryErrorIndex = CANNOT_FIND_COMPONENT_SERVICE
	Debug-Output "Cannot find component service"
	goto fatalregistry
    endif

    set OldVersionExisted = $(TRUE)

    set ValueName = ""
    set ValueData = ""
    set ValueStr  = ""
    set ValueList = {}

    ;
    ; Get the old values
    ;
    EnumRegValue $(KeyParameters) ValueList

    ForListDo $(ValueList)
	set ValueItem = $($)
	set ValueName = *($(ValueItem),1)
	set ValueData = *($(ValueItem),4)
	Ifstr(i) $(ValueName) == "INTERRUPT"
	    set IRQValue = $(ValueData)
		Debug-Output "OEMNADIN.INF: Registry IRQ: "$(IRQValue)
	else-ifstr(i) $(ValueName) == "IOADDRESS"
	    set IOAddrValue = $(ValueData)
		Debug-Output "OEMNADIN.INF: Registry IOAddr: "$(IOAddrValue)
	else-ifstr(i) $(ValueName) == "IoChannelReady"
	    set IOReadyValue = $(ValueData)
		Debug-Output "OEMNADIN.INF: Registry IOChannelReady: "$(IOReadyValue)
	else-ifstr(i) $(ValueName) == "Transceiver"
	    set TransceiverValue = $(ValueData)
		Debug-Output "OEMNADIN.INF: Registry Transceiver: "$(TransceiverValue)
	else-ifstr(i) $(ValueName) == "BusType"
	    set BusInterfaceType = $(ValueData)
	else-ifstr(i) $(ValueName) == "BusNumber"
	    set BusNumber = $(ValueData)
	endif
    EndForListDo

    ifstr(i) $(IRQValue) == ""
	set IRQValue = *($(IRQList), 2)
		Debug-Output "OEMNADIN.INF: Setting Default IRQ"
    endif
    ifstr(i) $(IOAddrValue) == ""
	set IOAddrValue = *($(IOAddrList), 1)
		Debug-Output "OEMNADIN.INF: Setting Default IOAddress"
    endif
    ifstr(i) $(IOReadyValue) == ""
	set IOReadyValue = *($(IOReadyListExt), 2)
		Debug-Output "OEMNADIN.INF: Setting Default IOChannelReady"
    endif
    ifstr(i) $(TransceiverValue) == ""
	set TransceiverValue = *($(TransceiverList), 4)
		Debug-Output "OEMNADIN.INF: Setting Default Transceiver"
    endif        
    
    set IOAddrValue = *($(IOAddrList), ~($(IOAddrValues),$(IOAddrValue)))
    set IRQValue = *($(IRQList), ~($(IRQList),$(IRQValue)))
    set IOReadyValue = *($(IOReadyListExt), $(IOReadyValue))
    set TransceiverValue = *($(TransceiverList), $(TransceiverValue))

;
;   Put up the adapter configuration dialog if necessary.
;
adaptersetup = +

    Debug-Output "At adaptersetup"
    Shell "" DebugConfiguration "before displaying dialog"

    
;    set IOAddrValue = *($(IOAddrList), ~($(IOAddrValues),$(IOAddrValue)))
;    set IRQValue = *($(IRQList), ~($(IRQList),$(IRQValue)))
;    set IOReadyValue = *($(IOReadyList), $(IOReadyValue))
;    set TransceiverValue = *($(TransceiverList), $(TransceiverValue))
;
    Shell "" DebugConfiguration "After List Translation"
    
    ;===================================================
    ;  Netcard Detection logic
    ;
    ;   Check that this card's parameters can be
    ;   fully detected.
    ;
    Shell $(ParamInf) Param_ParameterConfidence
    Ifstr(i) $($R0) != STATUS_SUCCESSFUL
	Debug-Output "OEMNADIN.INF: parameter confidence too low to bypass configuration"
	Goto adapteroptions
    Endif
    ;
    ;   If this is a detected card and we're in EXPRESS mode,
    ;   see if the parameters as they currently exist are
    ;   verifiably correct.
    ;
    Ifstr(i) $(DetectedCard) == TRUE
	Ifstr(i) $(!STF_INSTALL_MODE) != CUSTOM
	    Goto adapterverify
	Endif
    Endif
    ;
    ;  End Netcard Detection logic
    ;===================================================

adapteroptions = +
    Debug-Output "At adapteroptions"
    Set from = adapteroptions

;    set IOBaseAddrValue = *($(IOAddrList), ~($(IOAddrList),$(IOBaseAddrValue)))
;    set IOReadyValue = *($(IOReadyList), $(IOReady))
;    set TransceiverValue = *($(TransceiverList), $(Transceiver))

    read-syms FileDependentDlg$(!STF_LANGUAGE)

    ui start "InputDlg"

    ifstr(i) $(DLGEVENT) == "CONTINUE"
	  Set IRQValue = $(Combo1Out)
	     Set IOAddrValue = $(Combo2Out)
	Set IOReadyValue = ~($(IOReadyListExt),$(Combo3Out))
;        Set IOReadyValue = ~($(IOReadyList),$(Combo3Out))
	Set TransceiverValue = ~($(TransceiverList),$(Combo4Out))
	ui pop 1
    else-ifstr(i) $(DLGEVENT) == "BACK"
	set CommonStatus = STATUS_USERCANCEL
	Debug-Output "Action: exit. Bye."
	ui pop 1
	goto end
    else
	Debug-Output "Action: unknown. Bye."
	ui pop 1
	goto end
    endif
    
    ifstr(i) $(!STF_NCDETINFO) == {}
	Shell $(UtilityInf),GetBusTypeDialog,$(ProductHardwareDescription) $(BusInterfaceType) $(BusNumber)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif
	set BusInterfaceType = $($R1)
	set BusNumber = $($R2)
    else
	set BusInterfaceType = *($(!STF_NCDETINFO),5)
	set BusNumber = *($(!STF_NCDETINFO),6)
    endif

 aadapterverify = +

    Debug-Output "At adapterverify"
    Shell "" DebugConfiguration "after running dialog"

    ;===================================================
    ;  Netcard Detection logic
    ;
    ;   If this is a detected card, attempt to validate the options
    ;
    Ifstr(i) $(DetectedCard) != TRUE
	Goto skipoptions
    Endif

    Debug-Output "OEMNADIN.INF: Calling Param_VerifyCard"
    Shell $(ParamInf) Param_VerifyCard $(!STF_NCDETCARD)
    Ifstr(i) $($R0) == STATUS_SUCCESSFUL
	Debug-Output "OEMNADIN.INF: Param_VerifyCard succeeded"
	Goto skipoptions
    Endif
    ;
    ;   Give the user a chance to retry or force the options given.
    ;
    Set from = adapteroptions
    Set to = skipoptions
    Shell $(UtilityInf),RegistryErrorString,VERIFY_WARNING
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error: cannot get an error string."
	goto ShellCodeError
    endif
    set Error = $($R0)
    Goto Warning
    ;
    ;  End Netcard Detection logic
    ;===================================================

;
;   If installing, go create the necessary keys;
;   if configuring, they're already open.
;
skipoptions =+

    Debug-Output "At skipoptions"
    ifint $(OldVersionExisted) == $(TRUE)
	ifstr(i) $(!NTN_InstallMode) == configure
	    goto writeparameters
	endif
    endif
    StartWait
    ;
    ; Add Software Component
    ;
    ifint $(OldVersionExisted) == $(FALSE)
	ifstr(i) $(!NTN_InstallMode) == "install"
	   Ifstr(i) $(DoCopy) == "YES"

	      Shell $(UtilityInf), DoAskSource, $(!STF_CWDDIR), $(SrcDir) YES

	      Ifint $($ShellCode) != $(!SHELL_CODE_OK)
		  Goto ShellCodeError
	      Else-Ifstr(i) $($R0) == STATUS_FAILED
		  Shell $(UtilityInf) RegistryErrorString "ASK_SOURCE_FAIL"
		  ifint $($ShellCode) != $(!SHELL_CODE_OK)
		      goto ShellCodeError
		  endif
		  set Error = $($R0)
		  Goto fatal
	      Else-Ifstr(i) $($R0) == STATUS_USERCANCEL
		  Goto successful
	      Endif

	      Set SrcDir = $($R1)

	   Endif

	   install "Install-Option"
	   ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
	      Shell $(UtilityInf) RegistryErrorString "UNABLE_COPY_FILE"
	      ifint $($ShellCode) != $(!SHELL_CODE_OK)
		  goto ShellCodeError
	      endif
	      set Error = $($R0)
	      goto fatal
	   endif
	endif

	Debug-Output "At AddSoftwareComponent"
	Shell $(UtilityInf), AddSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareName), +
	    $(ProductSoftwareTitle), $(STF_CONTEXTINFNAME), +
	    $(ProductSoftwareImagePath), "kernel", "NDIS", {}, "",+
	    $(NetEventDLL)

	Set OEM_ABANDON_SOFTWARE = TRUE

	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif
	;
	;   At this point:
	;     $R1 contains the product version key handle;
	;     $R2 contains the NetRules subkey handle;
	;     $R3 contains the new Services key handle; and
	;     $R4 contains the Parameters key
	;     $R5 contains the Linkage Key
	;
	set RegistryErrorIndex = $($R0)
	set KeyProduct      = $($R1)
	Set SoftNetRulesKey = $($R2)
	CloseRegKey $($R3)
	CloseRegKey $($R4)
	CloseRegKey $($R5)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add software components"
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif

	set NewValueList = {{SoftwareType,$(NoTitle),$(!REG_VT_SZ),$(SoftwareType)},+
			   {MajorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMajorVersion)},+
			   {MinorVersion,$(NoTitle),$(!REG_VT_DWORD),$(ProductMinorVersion)},+
			   {Title,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareTitle)},+
			   {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareDescription)},+
			   {ServiceName,$(NoTitle),$(!REG_VT_SZ),$(ProductSoftwareName)},+
			   {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

	Debug-Output "At AddValueList - SoftwareType"
	Shell  $(UtilityInf), AddValueList, $(KeyProduct), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Registry error: add value list."
	    CloseRegKey $(KeyProduct)
	    CloseRegKey $(SoftNetRulesKey)
	    goto fatalregistry
	endif

	set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareType)},+
			    {use,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareUse)}, +
			    {bindform,$(NoTitle),$(!REG_VT_SZ),$(NetRuleSoftwareBindForm)}, +
			    {class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareClass)}, +
			    {bindable,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleSoftwareBindable)}, +
			    {InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

	Debug-Output "At AddValueList - bindform"
	Shell  $(UtilityInf), AddValueList, $(SoftNetRulesKey), $(NewValueList)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error."
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	CloseRegKey $(KeyProduct)
	CloseRegKey $(SoftNetRulesKey)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    EndWait
	    Debug-Output "Resgitry error: add value list."
	    goto fatalregistry
	endif
    endif
;
;   Create the HARDWARE\Netcard region and its corresponding service
;
    Debug-Output "At AddHardwareComponent"
    Shell $(UtilityInf), AddHardwareComponent, $(ProductHardwareName),$(STF_CONTEXTINFNAME),$(ProductKeyName)

    ifint $($R4) != -1
	Set OEM_ABANDON_OPTIONS = >($(OEM_ABANDON_OPTIONS), $(!NTN_SoftwareBase)"\Microsoft\Windows NT\CurrentVersion\NetworkCards\"$($R4))
    endif

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "Cannot add hardware component"
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	EndWait
	Debug-Output "Registry error: add hardware component"
	CloseRegKey $($R1)
	CloseRegKey $($R2)
	CloseRegKey $($R3)
	goto fatalregistry
    endif

;
;   At this point:
;     $R1  Registry key variable for HARDWARE\Netcard\(n)
;     $R2  Registry key variable for HARDWARE\Netcard\(n)\\NetRules
;     $R3  Registry key handle for <service>\Parameters key
;     $R4  Adapter number assigned to adapter
;     $R5  Service name generated by combining svc name with adapter number
;
    set KeyParameters = $($R3)
    set KeyAdapterRules = $($R2)
    set AdapterNumber = $($R4)

    set NewValueList = {{Manufacturer,$(NoTitle),$(!REG_VT_SZ),$(Manufacturer)},+
		       {Title,$(NoTitle),$(!REG_VT_SZ),"["$($R4)"] "$(ProductHardwareTitle)},+
		       {Description,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareDescription)},+
		       {ProductName,$(NoTitle),$(!REG_VT_SZ),$(ProductHardwareName)},+
		       {ServiceName,$(NoTitle),$(!REG_VT_SZ),$($R5)},+
		       {InstallDate,$(NoTitle),$(!REG_VT_DWORD),*($(Now),1)}}

    Debug-Output "At AddValueList - Manufacturer"
    Shell  $(UtilityInf), AddValueList, $($R1), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error"
	goto ShellCodeError
    endif

    CloseRegKey $($R1)

    set TempProdName = """"$(ProductHardwareName)$(AdapterNumber)""""
    set TempBindForm = $(TempProdName)$(NetRuleHardwareBindForm)

    set NewValueList = {{type,$(NoTitle),$(!REG_VT_SZ),$(NetRuleHardwareType)},+
			{bindform,$(NoTitle),$(!REG_VT_SZ),$(TempBindForm)}, +
			{class,$(NoTitle),$(!REG_VT_MULTI_SZ),$(NetRuleHardwareClass)}, +
			{InfOption,$(NoTitle),$(!REG_VT_SZ),$(Option)}}

    Debug-Output "At AddValueList - class"
    Shell  $(UtilityInf), AddValueList, $(KeyAdapterRules), $(NewValueList)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	EndWait
	Debug-Output "Resgitry error: add value list."
	CloseRegKey $(KeyParameters)
	CloseRegKey $(KeyAdapterRules)
	goto fatalregistry
    endif

    CloseRegKey $(KeyAdapterRules)

    goto writeparameters
;
;   REQUIRED:   $(KeyParameters) contains service Parameters key handle
;
writeparameters = +
    Debug-Output "At writeparameters"
;
;   Add the rest of the parameters to the Services area
;
    Ifstr(i) $(MachineType) == "MCA"
       set NewValueList = {{BusType,$(NoTitle),$(!REG_VT_DWORD),$(BusTypeNum)},+
		      {McaPosId,$(NoTitle),$(!REG_VT_DWORD),$(NETCARD_ID)},+
		      {SlotNumber,$(NoTitle),$(!REG_VT_DWORD),$(SlotNum)},+
		      {MediaType,$(NoTitle),$(!REG_VT_DWORD),1}}
    else                       
       Set IOAddrValue = *($(IOAddrValues), ~($(IOAddrList),$(IOAddrValue)))
       Shell "" DebugConfiguration "Before Writing Parameters"
       set NewValueList = {{INTERRUPT,$(NoTitle),$(!REG_VT_DWORD),$(IRQValue)},+
		      {BusType,$(NoTitle),$(!REG_VT_DWORD),$(BusInterfaceType)},+
		      {BusNumber,$(NoTitle),$(!REG_VT_DWORD),$(BusNumber)},+
		      {MediaType,$(NoTitle),$(!REG_VT_DWORD),1},+
		      {IoChannelReady,$(NoTitle),$(!REG_VT_DWORD),$(IOReadyValue)},+
		      {Transceiver,$(NoTitle),$(!REG_VT_DWORD),$(TransceiverValue)},+
		      {IOADDRESS,$(NoTitle),$(!REG_VT_DWORD),$(IOAddrValue)}}
    endif
    
    Shell  $(UtilityInf), AddValueList, $(KeyParameters), $(NewValueList)

    CloseRegKey $(KeyParameters)

    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error."
	goto ShellCodeError
    endif

    set RegistryErrorIndex = $($R0)

    Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	Debug-Output "Registry error: Add value list"
	goto fatalregistry
    endif

    EndWait

    goto successful

;-----------------------------------------------
; Binding section
;-----------------------------------------------
bindingadapter =+
    Debug-Output "At bindingadapter"
    set Error = "Binding: Sorry, not yet implemented."
    goto fatal

;-----------------------------------------------
; Removeadapter section
;-----------------------------------------------

removeadapter = +
    Debug-Output "At removeadapter"
    Ifstr(i) $(ProductKeyName) == $(!NTN_RegBase)
	; Remove Software Component
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    else
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $(!NTN_RegBase)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif

    goto end

;-----------------------------------------------
; Upgrade Software section
;-----------------------------------------------

UpgradeSoftware = +
    Debug-Output "At UpgradeSoftware"
    ;
    ; First determine whether we want to do upgrade or update for software
    ; or hardware component. Then we will determine whether the Mode is
    ; update or upgrade.
    ;
    ; If the same version of the product existed in the registry, we do
    ; update. Otherwise, we will do a upgrade
    ;
    OpenRegKey $(!REG_H_LOCAL) "" $(ProductKeyName) $(MAXIMUM_ALLOWED) KeyProduct
    Ifstr $(KeyProduct) != $(KeyNull)
	install "Install-Update"
	ifstr(i) $(STF_INSTALL_OUTCOME) != STF_SUCCESS
	    goto fatal
	endif
	SetRegValue $(KeyProduct) {MajorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMajorVersion)}
	SetRegValue $(KeyProduct) {MinorVersion,$(NoTitle),$(!REG_VT_SZ),$(ProductMinorVersion)}
	CloseRegKey $(KeyProduct)
    else
	goto fatalregistry
    endif

    goto end
    ;
    ; End of Upgrade Software
    ;

;
;  Escape hatches
;
successful = +
    Debug-Output "At successful"
    goto end

abandon = +
    Debug-Output "At abandon"
    ForListDo $(OEM_ABANDON_OPTIONS)
	Shell $(UtilityInf), RemoveHardwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), $($)
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    EndForListDo

    Ifstr(i) $(OEM_ABANDON_SOFTWARE) == TRUE
	; Remove Software Component
	Shell $(UtilityInf), RemoveSoftwareComponent, $(Manufacturer), +
	    $(ProductSoftwareName), FALSE
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    Debug-Output "ShellCode error"
	    goto ShellCodeError
	endif

	set RegistryErrorIndex = $($R0)

	Ifstr(i) $(RegistryErrorIndex) != NO_ERROR
	    goto fatalregistry
	endif
    endif

    goto end

;
; warning display
;
warning = +
    Debug-Output "At warning"
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "WARNING", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(to)
    else-ifstr(i) $($R1) == "CANCEL"
	goto $(from)
    else
	goto "end"
    endif
;
; non fatal error display
;
nonfatalinfo = +
    Debug-Output "At nonfatalinfo"
    Set Severity = STATUS
    Set CommonStatus = STATUS_USERCANCEL
    goto nonfatalmsg
nonfatal = +
    Debug-Output "At nonfatal"
    Set Severity = NONFATAL
    goto nonfatalmsg
nonfatalmsg = +
    Debug-Output "At nonfatalmsg"
    ifstr(i) $(Error) == ""
	Set Severity = NONFATAL
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), $(Severity), $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    ifstr(i) $($R1) == "OK"
	goto $(from)
    else
	goto "end"
    endif

;
;  Registry is broken
;
fatalregistry = +
    Debug-Output "At fatalregistry"
    Shell $(UtilityInf) RegistryErrorString $(RegistryErrorIndex)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif
    set Error = $($R0)
    goto fatal
;
;  Netcard detection failure
;
fataldetect = +
    Debug-Output "At fataldetect"
    Shell $(UtilityInf),RegistryErrorString,CANNOT_DETECT
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	Debug-Output "ShellCode error: cannot get an error string."
	goto ShellCodeError
    endif
    set Error = $($R0)
    Goto fatal
;
; fatal error display
;
fatal = +
    Debug-Output "At fatal"
    ifstr(i) $(Error) == ""
	Shell $(UtilityInf) RegistryErrorString "SETUP_FAIL"
	ifint $($ShellCode) != $(!SHELL_CODE_OK)
	    goto ShellCodeError
	endif
	set Error = $($R0)
    endif
    Shell $(subroutineinf) SetupMessage, $(!STF_LANGUAGE), "FATAL", $(Error)
    ifint $($ShellCode) != $(!SHELL_CODE_OK)
	goto ShellCodeError
    endif

    goto setfailed

;
;  Shelling error
;
ShellCodeError = +
    Debug-Output "At ShellCodeError"
    set DlgType      = "MessageBox"
    set STF_MB_TITLE = "Error: "$(FunctionTitle)
    set STF_MB_TEXT  = "Shell Code Error"
    set STF_MB_TYPE  = 1
    set STF_MB_ICON  = 3
    set STF_MB_DEF   = 1
    ui start "Error Message"
    goto setfailed

setfailed = +
    Debug-Output "At setfailed"
    set CommonStatus = STATUS_FAILED
    ;
    ; if OEM_ABANDON_ON == TRUE, then remove the registry entries
    ;
    ifstr(i) $(OEM_ABANDON_ON) == TRUE
	set OEM_ABANDON_ON = FALSE
	goto abandon
    endif
    goto end

end = +
    Debug-Output "At end"
    goto term

term = +
    Debug-Output "At term"
    Return $(CommonStatus)


[DebugConfiguration]

    Set InfName = "OEMNADIN.INF"
    Debug-Output $(InfName)" **CONFIGURATION STATE: "$($0)
    Debug-Output $(InfName)" IRQValue is "$(!p:IRQValue)
    Debug-Output $(InfName)" IOAddrValue is "$(!p:IOAddrValue)
    Debug-Output $(InfName)" IOReadyValue is "$(!p:IOReadyValue)
    Debug-Output $(InfName)" TransceiverValue is "$(!p:TransceiverValue)

    return


;***************************************************************
;  INSTALL SECTIONS
;***************************************************************
[Install-Option]
    Debug-Output "At Install-Option"
    set STF_VITAL = ""

    ifstr(i) $(AddCopy) == "YES"

	;
	; Add the files to the copy list
	;
	;  BUGBUG: eliminate the "nt2" in the next line when Sunil fixes
	;      the other INF files
	;
	AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers

    endif

    ifstr(i) $(DoCopy) == "YES"

       ;
       ; Copy files in the copy list
       ;
       set !STF_NCPA_FLUSH_COPYLIST = TRUE
       CopyFilesInCopyList

    endif

    Exit

[Install-Update]
    Debug-Output "At Install-Update"
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   ;set STF_VERSION     = "YES"

   AddSectionFilesToCopyList Files-$(Option) $(SrcDir) $(!STF_WINDOWSSYSPATH)\drivers
   CopyFilesInCopyList

   exit

[Install-Helpfile]
   Debug-Output "At Install-Helpfile"
   set STF_VITAL        = ""
   set STF_OVERWRITE    = "VERIFYSOURCEOLDER"
   ;set STF_VERSION     = "YES"
    set !STF_NCPA_FLUSH_COPYLIST = TRUE
    
   AddSectionFilesToCopyList Files-hlp $(SrcDir) $(!STF_WINDOWSSYSPATH)
   CopyFilesInCopyList

   exit

